Circular no. **842(C)** Date: 05.09.2019

Guideline rates for undertaking layout works and other minor works given are being revised as under:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| S. No. | Item Description | Size | Rate | Units |
|  | Laying HDPE pipes | 1” to 3” | 10/- | Per meter |
|  | Butt Joints for HDPE pipes | Upto 1”  | 200/- | Each |
|  | Butt Joints for HDPE pipes | Upto 2” | 300/- | Each |
|  | Butt Joints for HDPE pipes | Upto 3” | 400/- | Each |
|  | CC pipe laying | 6”/8” | 18/- | Rft |
|  | SWG pipes laying | 8” | 20/- | Rft |
|  | SWG pipes laying | 4” to 6” | 15/- | Rft |
|  | GI Pipe works | 3” / 4” | 15 / 20/- | Rft |
|  | GI Pipe works | 2” to 2 ½” | 13/- | Rft |
|  | GI Pipe works | ½ to 1 ½” | 11/- | Rft |
|  | Gate wall fixing | 3” to 4” | 500/- | No. |
|  | Gate wall fixing | ½ to 2” | 65/- | No. |
|  | Laying PVC pipe  | Upto 4” | 14/ | Rft |
|  | Laying PVC pipe  | Upto 3” | 12/- | Rft |
|  | Laying PVC pipe  | Upto 2”  | 10/- | Rft |
|  | Drainage Man holes – with table brick | 1’ to 3’6” depth | 750/- | Nos. |
|  | Drainage Man holes – with table brick | 4’ to 6’ depth | 1,000/- | Nos. |
|  | Square Man holes – with/without CC cover | 3’x 3’x 3’/4’ | 800/1,200/- |  |
|  | Square Man holes – with/without CC cover | 4/5’x 4/5’x 4/5’ | 1,000/1,500/- |  |
|  | Small square Man holes | 2’x2’x 2’/3’ | 500/- | Nos. |
|  | Small square Man holes | 18” x 18” x 2’/3’ | 300/- | Nos. |
|  | Open well submersible or mono block pump fitting with NRV | -- | 1,000/- | Per No. |
|  | Laying of C.C. pipe (Hume) | Upto 1’ | 20/- | Rft |
|  | Laying of C.C. pipe (Hume) | Upto 2’ | 26/-  | Rft |
|  | Tub fixing | -- | 1,200/- | No. |
|  | Fixing of Syntax tanks | -- | 0.60/- | Per liter |
|  | Loft tank connections | Upto 200 ltrs | 600/- | Per No. |
|  | PVC bends & fittings | 3” & 4” | 30 /- | Per No. |
|  | Nani Trap | 3” & 4” | 60/- | Per No. |
|  | Eco drain pipe laying | 4” /6”  | 12/- | Rft  |
|  | Eco drain pipe laying | 8”  | 20/- | Rft  |
|  | Eco drain pipe laying – pipes + manholes + gully traps – without excavation | 4”to 8” | 25/- | Rft |
|  | Submersible pump fixing.New upto 300 ft.New beyond 300 ft.Removal upto 300ft.Removal beyond 300 ft.Refixing upto 300 ft.Refixing beyond 300 ft. Removal/refixing with chain pulley  | 3,000/-10/- per rft extra1,500/-Rs. 4/- per rft extra1,000/-Rs. 3/- per rft extra2,000/- extra |  |  |

These rates shall be applicable for all sites where these works have started after 06 September, 2019.

Managing Director.