Old Intl Memo No. 912/39/ New circular no. **886(b)** Date. 05.04.2017

Sub.: Design for RCC gate pillars & compound wall.

All gates must have RCC columns on both sides. Unless otherwise specified by the architect/structural engineer, gate pillars shall be made as per design enclosed.

Wherever possible use normal footings. However, at the boundaries with neighboring land use shoe footing as per drawing. For purposes of marking of boundary, roads and plots use corner footing as given in drawing.

Hereafter all compound walls shall be in RCC (column and plinth beam only) with hollow block filling. Compound wall will be made as per design given herein and shall be suitably covered in brick and plaster as per architectural drawings.

Relaxation has been given here to make pit size equal to the size of proposed footing. Centring boxes for sides of footings need not be used.

Relevant drawing is attached is figure 18 & 19 in circular 889(a)

Soham Modi.