Internal Memo No. 912/49 – Construction Division Date: 24.12.2010

Sub.:– Kitchen platform corrections and black oxide filling.

In case where the kitchen platform RCC slab is casted 1 or 2” below the desired level correction needs to be made as shown in the plan. The vertical granite band should be exactly 4” thick. Make a groove as shown in the plan so that the platform projection behind the granite band can be covered by wood work.

Black oxide filling: Clean the grooves between granite joints to a depth of about 2 or 3 mm. Fill with a paste of cement or black oxide mixed in a proportion of 2:1. Wait for a couple of hours before wiping it clean with a damp sponge.

Plan enclosed.

Soham Modi