Intl Memo no. **912/87 -** Construction Date: 01.04.2016

Sub.: Design for door frames.

1. Door frame sizes should be standardized as given under.
   1. Main doors of flats, villas and farms should be 3’6” wide with a frame size of 5”x 3” along with threshold.
   2. Bedroom (and for large sitouts) doors of flats, villas and farms should be 3’wide with a frame size of 4 ½” x 2 1/2” along without threshold.
   3. Bathroom, storeroom, balcony, utility and other doors of flats, villas and farms should be 2’6” wide with a frame size of 4 ½” x 2 1/2” along without threshold.
   4. All external doors must have a threshold.
   5. The design for the door frame including threshold is attached herein. Design to be followed across all sites.
2. Unless otherwise specified the above to be strictly followed.
3. Project managers/engineers to bring to notice of MD if any discrepancies in the above by email. Nagalaxmi shall ensure that working drawings comply with the above before issuing.

Soham Modi.