Intl Memo no. **912/91 -** Construction Date: 16.03.2016

Sub.: Installation of mosquito mesh.

We have received requests from customers for installation of mosquito mesh on the main door. Hereafter, the standard policy shall be as under.

Installation of mosquito mesh shutter shall be permitted across all projects. However, in the overall interest of maintaining uniform look and feel, the mosquito mesh on the main door can be installed subject to the following conditions:

1. The mosquito mesh should be made in wood or aluminium and painted/ polished in dark brown colour.
2. The mesh can be sliding. In apartment complexes, in case it is openable type, the mesh should be openable by 180 degrees, so that it does not obstruct the passage.
3. MS grills or aluminium grills cannot be installed.
4. In case of villas such a mesh will be permitted external doors.
5. In case of sliding windows, 3 track windows with mosquito mesh can be provided at additional cost. In case of openable windows, roll down mosquito mesh can be provided at additional cost.

Soham Modi.