Circular No. **827(b)** Date: 17.05.2017

Sub.: Guide line rates for making hoardings

We have standardized the hoarding design by 6’x4’ and 8’x12’ hoardings. Several hundred such hoardings may be required. The guidelines rates for making these hoardings shall be as follows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| S.No. | Description of work | Hoarding size | Rate | units |
| 1. | Fabrication | 6’x4’ | 600 | Nos. |
| 2. | Fabrication | 8’x12’ | 900 | Nos. |
| 3. | Painting- 1 coat redoxide | 6’x4’ | 100 | Nos. |
| 4. | Painting- 1 coat redoxide | 8’x12’ | 150 | Nos. |
| 5. | Painting- 1 coat redoxide + 2 coats enamel | 6’x4’ | 200 | Nos. |
| 6. | Painting- 1 coat redoxide + 2 coats enamel | 8’x12’ | 350 | Nos. |
| 12. | Civil works for fixing boards including mason and helper excluding transport cost | 6’x4’ | 300 | Nos. |
| 13. | Civil works for fixing boards including mason and helper excluding transport cost | 8’x12’ | 500 | Nos. |

Note: Flex to be fixed by Murali (promotions) with help of department labour from site.

Soham Modi