Internal memo no. 912/139/A - Construction division Date: 11-03-2022

Subject: List of standard size of door frames & door shutters

Key words: door frame size, door shutter size.

1. A standardised list of door frames and door shutters is given in annexure -A herein.
2. Following types of doors and door frames are to be used.
3. WPC or wooden door frame. This is to be installed at time of civil work. Door shutters to be installed after completion of civil work.
4. Fire door – here opening to be left in civil work of larger size. After completion of civil work granite soffit to be fixed on all 4 sides to exact dimension + 6mm margin for easy fit.
5. UPVC French windows – here opening to be left in civil work of larger size. After completion of civil work granite soffit to be fixed on all 4 sides to exact dimension + 6mm margin for easy fit.
6. Toughened glass doors – here opening to be left in civil work of larger size. After completion of civil work granite soffit to be fixed on all 4 sides. Vendor to consider dimension after fitting granite soffit.
7. MS hose cabinet – opening to be left in civil work. Cabinet to be fixed after completion of civil work. This is to be primarily used for commercial projects.
8. For all new projects dimensions will be specified in mm. Accordingly this circular to be modified (eg.: 7ft x 3ft door frame would be resized to 2150 x 900mm).
9. Hereafter all requisitions to be made as per code given herein.
10. All new working drawings must use this code.

Soham Modi.