Internal memo no. 903/25 - purchase division Date: 20.09.2018

Subject: Electric power supply - use of plastic boxes.

At the moment MS boxes are being used to house distribution boards (db), starters, circuit breakers, isolators, timers, switches, etc. Life of MS boxes is poor and may get electrified due to loose connections. Therefore, from hereon plastic boxes (Sintex brand or equivalent) shall be used in place of MS boxes. The plastic boxes may be fixed to compound wall or independently erected using a frame of 1.5” MS sq box section or L angle. The boxes must be locked with a padlock. The details of the boxes and the uses are given below.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Sl. No. | Item no. | Box size | Rate per box in Rs. | To be used for |
|  | GSJB 2014 | 9”x 6”x 5” | 410 | Use for fixing small starters, switches, timers or isolator  |
|  | GSJB 2817 | 11”x 6.5”x 5” | 650 | Use for fixing small starters, switches, timers or isolator |
|  | GSJB 3525 | 14”x 10”x 6” | 1,000 | For single phase 4/8 way DB or electronic starter for pumps |
|  | GSJB 4030 | 15”x 11”x 7” | 1,100 | For 3 phase 4 way DB. |
|  | GSJB 4537 | 18”x 14”x 9” | 1,300 | For 3 phase 8 way DB. |
|  | GSJB 7450 | 27”x 19”x 8” | 4,850 | For 3 phase in and 3 phase out, 8 way DB box used for generator connection in flats. |

Soham Modi