Circular No. **805(C)** Date: 24-09-2021

Sub.: Revised Guideline rates for Civil works – Apartments - Lumpsum

|  |  |  |  |
| --- | --- | --- | --- |
| S. No | Description | Rate (Rs.) | Units |
| 1. | Apartments turnkey civil work charges including brick work, plastering, shelves/ lofts upto 100 sft., elevation, ducts, internal scaffolding tying and removing, stilt floor plastering, sand screening, curing, lifting charges, floor chipping, batana shifting for flooring, skirting plastering, holes closing, minor finishing works, electrical holes closing, water tank plastering, railing fixing, doors frames, ventilators and template fixing, rooms and stilt floors, lift rooms, etc. Rate applicable upto 5 floors. For upper floors additional rate shall be Rs. 10/- per sft extra.  Excludes compound wall, roads and common amenities works. | 115.00  20.00  20.00 | Per sft. for each floor  Per sft. for Stilt floor  Terrace floor |
| 2. | Stage wise billing shall be made as follows:  Brick work including common areas -Rs. 40/- per sft  Elevation work – Rs. 25/- per sft  Internal Plastering (2 coats) including corridors – Rs. 30/- per sft.  Holes closing, floor chipping and dust shifting including common areas - Rs.10/- per sft (this work can be out sourced to earth work contractors @ Rs. 7/- per sft – balance Rs. 3/- can be paid to civil contractors)  Final finishing works including skirting, plastering, edges rebuilding, etc. – Rs. 10/- per sft.  Terrace floor finishing works – Rs. 20/- per sft of terrace area  Stilt floor plastering and minor finishing works including level marking and dust shifting for flooring – Rs.20/- per sft.  For upper floor beyond 5 floors Rs. 10/- per sft can be paid extra in ratio of 4:3:3 for brick work, internal plastering and external plastering. |  |  |

Notes:

1. All labour and equipment to be provided by contractor.
2. The above rates include hacking charges.
3. If charges for hacking, tying, removing, scaffolding, chipping, shifting mortar for flooring, etc., are paid to other contractors, ensure that these payments are either debited to the contractors account or the bill amount is appropriately reduced.
4. The rates exclude external scaffolding, tying and removing.
5. Rates shall be applicable for new projects only. Consider these rates for estimate of GHT & BRGV.
6. For clubhouse of 3 to 5 floors the rate shall be Rs. 85/- per floor in place of Rs. 115/- as scope of work is lesser. Ceiling plastering may be avoided in clubhouse in all areas except staircase, lobby, bathrooms and top floors.

Managing Director.